Put a neodinium magnet to the knob part of the grip and close it with a M4 threaded insert.

You can use the cnob as a screwdriver.

